{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Setting","Protocol(Ext)","Protocol(Short)","Protocol(Raw)","Dictionary(Ext)","Dictionary(Short)","Raw"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Setting","index":0,"n_rows":6,"n_cols":2,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[null,"Hardware Target : KIMM220602"]
[null,"@MASS\n# | Delay : [sec] | Load Follow : Off(0) / On(1) | $a : Stoic Ratio | $a : Min Flow | $a : Set Flow\n$a | [AN] H2 | [AN] N2 | [AN(NH3)] HN3 | [AN(NH3)] N2 | [CA] Air | [CA] N2\n\n@HUM&TEMP\n# | Delay : [sec] | Relative Humidity : Off(0) / On(1) | $a : Path | $a : Relative Humidity | $a : Bottle Temp | $b : Cell Temp | $b : P.Heater Temp\n$a | [AN] Wet | [AN(NH3)] Wet | [CA] Wet\n$b | [CELL] \n\n@BP\n# | Delay : [sec] | Different BP : Off(0) / On(1) | $a : Back Pressure | $a : Outlet?\n$a | [Anode]  | [Cathode] \n\n@LOAD\n# | Delay: [sec] | Target : V(0) / I(1) / P(2) | Mode : Cnst(0) / Trip(1) | Cnst : Value | Trip : One(0) / Round(1) | Trip : Initial | Trip : From | Trip : To | Trip : Final | Trip : dValue | Trip : dT [sec]"]

{"sheet":"Protocol(Ext)","index":1,"n_rows":1,"n_cols":51,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
[null,"Delay\r\n[sec]","Load Follow\r\nOff(0)/On(1)","[AN] H2\r\nStoic Ratio","[AN] N2\r\nStoic Ratio","[AN(NH3)] HN3\r\nStoic Ratio","[AN(NH3)] N2\r\nStoic Ratio","[CA] Air\r\nStoic Ratio","[CA] N2\r\nStoic Ratio","[AN] H2\r\nMin Flow","[AN] N2\r\nMin Flow","[AN(NH3)] HN3\r\nMin Flow","[AN(NH3)] N2\r\nMin Flow","[CA] Air\r\nMin Flow","[CA] N2\r\nMin Flow","[AN] H2\r\nSet Flow","[AN] N2\r\nSet Flow","[AN(NH3)] HN3\r\nSet Flow","[AN(NH3)] N2\r\nSet Flow","[CA] Air\r\nSet Flow","[CA] N2\r\nSet Flow","Delay\r\n[sec]","Relative Humidity\r\nOff(0)/On(1)","[AN] Wet\r\nPath","[AN(NH3)] Wet\r\nPath","[CA] Wet\r\nPath","[AN] Wet\r\nRelative Humidity","[AN(NH3)] Wet\r\nRelative Humidity","[CA] Wet\r\nRelative Humidity","[AN] Wet\r\nB.Temp.","[AN(NH3)] Wet\r\nB.Temp.","[CA] Wet\r\nB.Temp.","[CELL]\r\nC.Temp.","[CELL]\r\nP.H.Temp.","Delay\r\n[sec]","Different BP\r\nOff(0)/On(1)","[Anode]\r\nBack Pressure","[Cathode]\r\nBack Pressure","[Anode]\r\nOutlet","[Cathode]\r\nOutlet","Delay: [sec]","Target\r\nV(0) / I(1) / P(2)","Mode\r\nCnst(0) / Trip(1)","Cnst\r\nValue","Trip\r\nOne(0) / Round(1)","Trip\r\nInitial","Trip\r\nFrom","Trip\r\nTo","Trip\r\nFinal","Trip\r\ndValue","Trip\r\ndT [sec]"]

{"sheet":"Protocol(Short)","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Protocol(Raw)","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Dictionary(Ext)","index":4,"n_rows":4,"n_cols":51,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["MASS","Delay : [sec]","Load Follow : Off(0) / On(1)","[AN] H2 : Stoic Ratio","[AN] N2 : Stoic Ratio","[AN(NH3)] HN3 : Stoic Ratio","[AN(NH3)] N2 : Stoic Ratio","[CA] Air : Stoic Ratio","[CA] N2 : Stoic Ratio","[AN] H2 : Min Flow","[AN] N2 : Min Flow","[AN(NH3)] HN3 : Min Flow","[AN(NH3)] N2 : Min Flow","[CA] Air : Min Flow","[CA] N2 : Min Flow","[AN] H2 : Set Flow","[AN] N2 : Set Flow","[AN(NH3)] HN3 : Set Flow","[AN(NH3)] N2 : Set Flow","[CA] Air : Set Flow","[CA] N2 : Set Flow"]
["HUM&TEMP"," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," ","Delay : [sec]","Relative Humidity : Off(0) / On(1)","[AN] Wet : Path","[AN(NH3)] Wet : Path","[CA] Wet : Path","[AN] Wet : Relative Humidity","[AN(NH3)] Wet : Relative Humidity","[CA] Wet : Relative Humidity","[AN] Wet : Bottle Temp","[AN(NH3)] Wet : Bottle Temp","[CA] Wet : Bottle Temp","[CELL] : Cell Temp","[CELL] : P.Heater Temp"]
["BP"," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," ","Delay : [sec]","Different BP : Off(0) / On(1)","[Anode] : Back Pressure","[Cathode] : Back Pressure","[Anode] : Outlet","[Cathode] : Outlet"]
["LOAD"," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," ","Delay: [sec]","Target : V(0) / I(1) / P(2)","Mode : Cnst(0) / Trip(1)","Cnst : Value","Trip : One(0) / Round(1)","Trip : Initial","Trip : From","Trip : To","Trip : Final","Trip : dValue","Trip : dT [sec]"]

{"sheet":"Dictionary(Short)","index":5,"n_rows":4,"n_cols":21,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["MASS","Delay : [sec]","Load Follow : Off(0) / On(1)","[AN] H2 : Stoic Ratio","[AN] N2 : Stoic Ratio","[AN(NH3)] HN3 : Stoic Ratio","[AN(NH3)] N2 : Stoic Ratio","[CA] Air : Stoic Ratio","[CA] N2 : Stoic Ratio","[AN] H2 : Min Flow","[AN] N2 : Min Flow","[AN(NH3)] HN3 : Min Flow","[AN(NH3)] N2 : Min Flow","[CA] Air : Min Flow","[CA] N2 : Min Flow","[AN] H2 : Set Flow","[AN] N2 : Set Flow","[AN(NH3)] HN3 : Set Flow","[AN(NH3)] N2 : Set Flow","[CA] Air : Set Flow","[CA] N2 : Set Flow"]
["HUM&TEMP","Delay : [sec]","Relative Humidity : Off(0) / On(1)","[AN] Wet : Path","[AN(NH3)] Wet : Path","[CA] Wet : Path","[AN] Wet : Relative Humidity","[AN(NH3)] Wet : Relative Humidity","[CA] Wet : Relative Humidity","[AN] Wet : Bottle Temp","[AN(NH3)] Wet : Bottle Temp","[CA] Wet : Bottle Temp","[CELL] : Cell Temp","[CELL] : P.Heater Temp"]
["BP","Delay : [sec]","Different BP : Off(0) / On(1)","[Anode] : Back Pressure","[Cathode] : Back Pressure","[Anode] : Outlet","[Cathode] : Outlet"]
["LOAD","Delay: [sec]","Target : V(0) / I(1) / P(2)","Mode : Cnst(0) / Trip(1)","Cnst : Value","Trip : One(0) / Round(1)","Trip : Initial","Trip : From","Trip : To","Trip : Final","Trip : dValue","Trip : dT [sec]"]

{"sheet":"Raw","index":6,"n_rows":97,"n_cols":4,"rows_kept":97,"cut":false,"hidden":false,"merged":[]}
["@HUM&TEMP","0"]
["#Target","Off(0) / On(1)"]
["Relative Humidity","1"]
["#Target","Path","Relative Humidity","Bottle Temp"]
["[AN] Wet","1","800.00","0.00"]
["[AN(NH3)] Wet","1","0.00","0.00"]
["[CA] Wet","1","70.00","0.00"]
["#Target","Cell Temp","P.Heater Temp"]
["[CELL]","90.00","95.00"]
["#Target","[sec]"]
["Delay","20.00"]
["@MASS","1"]
["#Target","Off(0) / On(1)"]
["Load Follow","0"]
["#Target","Stoic Ratio","Min Flow","Set Flow"]
["[AN] H2","0.00","0.00","700.00"]
["[AN] N2","0.00","0.00","0.00"]
["[AN(NH3)] HN3","0.00","0.00","0.00"]
["[AN(NH3)] N2","0.00","0.00","0.00"]
["[CA] Air","0.00","0.00","900.00"]
["[CA] N2","0.00","0.00","600.00"]
["#Target","[sec]"]
["Delay","10.00"]
["@BP","2"]
["#Target","Off(0) / On(1)"]
["Different BP","0"]
["#Target","Back Pressure","Outlet"]
["[Anode]","60.00","1"]
["[Cathode]","60.00","1"]
["#Target","[sec]"]
["Delay","10.00"]
["@MASS","3"]
["#Target","Off(0) / On(1)"]
["Load Follow","0"]
["#Target","Stoic Ratio","Min Flow","Set Flow"]
["[AN] H2","0.00","0.00","0.00"]
["[AN] N2","0.00","0.00","2000.00"]
["[AN(NH3)] HN3","0.00","0.00","0.00"]
["[AN(NH3)] N2","0.00","0.00","0.00"]
["[CA] Air","0.00","0.00","0.00"]
["[CA] N2","0.00","0.00","2000.00"]
["#Target","[sec]"]
["Delay","8.00"]
["@MASS","4"]
["#Target","Off(0) / On(1)"]
["Load Follow","0"]
["#Target","Stoic Ratio","Min Flow","Set Flow"]
["[AN] H2","0.00","0.00","700.00"]
["[AN] N2","0.00","0.00","0.00"]
["[AN(NH3)] HN3","0.00","0.00","0.00"]
["[AN(NH3)] N2","0.00","0.00","0.00"]
["[CA] Air","0.00","0.00","1500.00"]
["[CA] N2","0.00","0.00","0.00"]
["#Target","[sec]"]
["Delay","50.00"]
["@MASS","5"]
["#Target","Off(0) / On(1)"]
["Load Follow","0"]
["#Target","Stoic Ratio","Min Flow","Set Flow"]
["[AN] H2","0.00","0.00","0.00"]
["[AN] N2","0.00","0.00","0.00"]
["[AN(NH3)] HN3","0.00","0.00","0.00"]
["[AN(NH3)] N2","0.00","0.00","0.00"]
["[CA] Air","0.00","0.00","0.00"]
["[CA] N2","0.00","0.00","0.00"]
["#Target","[sec]"]
["Delay","5.00"]
["@HUM&TEMP","6"]
["#Target","Off(0) / On(1)"]
["Relative Humidity","1"]
["#Target","Path","Relative Humidity","Bottle Temp"]
["[AN] Wet","1","0.00","0.00"]
["[AN(NH3)] Wet","1","0.00","0.00"]
["[CA] Wet","1","0.00","0.00"]
["#Target","Cell Temp","P.Heater Temp"]
["[CELL]","0.00","0.00"]
["#Target","[sec]"]
["Delay","7.00"]
["@HUM&TEMP","7"]
["#Target","Off(0) / On(1)"]
["Relative Humidity","1"]
["#Target","Path","Relative Humidity","Bottle Temp"]
["[AN] Wet","0","0.00","0.00"]
["[AN(NH3)] Wet","1","0.00","0.00"]
["[CA] Wet","0","0.00","0.00"]
["#Target","Cell Temp","P.Heater Temp"]
["[CELL]","0.00","0.00"]
["#Target","[sec]"]
["Delay","7.00"]
["@BP","8"]
["#Target","Off(0) / On(1)"]
["Different BP","0"]
["#Target","Back Pressure","Outlet"]
["[Anode]","0.00","1"]
["[Cathode]","0.00","1"]
["#Target","[sec]"]
["Delay","3.50"]